# Projections Transform List

- Albers Equal-Area Conic
- Azimuthal Equidistant
- Cassini-Soldner
- Cylindrical Equal Area
- Eckert IV
- Eckert VI
- Equidistant Conic
- Equidistant Cylindrical
- Equirectangular
- Gauss-Kruger
- Gall Stereographic
- GEOS - Geostationary Satellite View
- Gnomonic
- Hotine Oblique Mercator
- Krovak
- Laborde Oblique Mercator
- Lambert Azimuthal Equal Area
- Lambert Conic Conformal (1SP)
- Lambert Conic Conformal (2SP)
- Lambert Conic Conformal (2SP Belgium)
- Lambert Cylindrical Equal Area
- Mercator (1SP)
- Mercator (2SP)
- Miller Cylindrical
- Mollweide
- New Zealand Map Grid
- Oblique Mercator
- Oblique Stereographic
- Orthographic
- Polar Stereographic
- Polyconic
- Robinson
- Rosenmund Oblique Mercator
- Sinusoidal
- Swiss Oblique Cylindrical
- Swiss Oblique Mercator
- Stereographic
- Transverse Mercator
- Transverse Mercator (Modified Alaska)
- Transverse Mercator (South Oriented)
- Tunisia Mining Grid
- VanDerGrinten

## Related Material

- Random Outstanding Issues
- Projection Documentation Principles
- EPSG Geodesy Web Page, with EPSG projection database used to generate libgeotiff normalization csv files.
- EPSG Guidance Note # 7: Describes various projection formulas, and some background information.
- Wkt_adam.zip: Text file relating EPSG PCS/GCS codes to OpenGIS WKT representations, courtesy of Adam Gawne-Cain of Cadcorp.
- OGC WKT Coordinate System Issues
- MapRef