# New Zealand Map Grid

Name | New Zealand Map Grid EPSG Code | 9811
GeoTIFF Code | CT_NewZealandMapGrid (26)
OGC WKT Name | New_Zealand_Map_Grid
Supported By | EPSG, GeoTIFF, PROJ.4

### Projection Parameters

Name | EPSG # | GeoTIFF ID | OGC WKT | Units | Notes Latitude of natural origin | 1 | NatOriginLat | latitude_of_origin | Angular |
Longitude of natural origin | 2 | NatOriginLong | central_meridian | Angular |
False Easting | 6 | FalseEasting | false_easting | Linear |
False Northing | 7 | FalseNorthing | false_northing | Linear |

### PROJ.4 Organization

      +proj=nzmg  +lat_0=Latitude of natural origin
                  +lon_0=Longitude of natural origin
                  +x_0=False Easting
                  +y_0=False Northing

### EPSG Notes

New Zealand Department of Lands technical circular 1973/32.